Uses of Interface org.ocap.si.TableChangeListener

Overview | Package | Class | Use | Tree | Deprecated | Index | Help

PREV NEXT | FRAMES NO FRAMES

## Uses of Interface
org.ocap.si.TableChangeListener

Packages that use TableChangeListener
org.ocap.si | The org.ocap.si package represents MPEG-2 PSI data.

Uses of TableChangeListener in org.ocap.si

Methods in org.ocap.si with parameters of type TableChangeListener
`abstract void` | `ProgramMapTableManager.addInBandChangeListener(TableChangeListener listener, Locator locator)` Add a TableChangeListener object that will be notified when the inband PMT changes.
`abstract void` | `ProgramAssociationTableManager.addInBandChangeListener(TableChangeListener listener, Locator locator)` Add a TableChangeListener object that will be notified when the inband PAT for the channel (transport stream) identified by the Locator parameter changes.
`abstract void` | `ProgramAssociationTableManager.addOutOfBandChangeListener(TableChangeListener listener)` Add a TableChangeListener object that will be notified when the out-of-band PAT changes.
`abstract void` | `ProgramMapTableManager.addOutOfBandChangeListener(TableChangeListener listener, int programNumber)` Add a TableChangeListener object that will be notified when the out-of-band PMT changes.
`abstract void` | `ProgramMapTableManager.removeInBandChangeListener(TableChangeListener listener)` Remove the TableChangedListener object for the inband PMT.
`abstract void` | `ProgramAssociationTableManager.removeInBandChangeListener(TableChangeListener listener)` Remove the TableChangeListener object for the inband PAT.
`abstract void` | `ProgramMapTableManager.removeOutOfBandChangeListener(TableChangeListener listener)` Remove the TableChangedListener object for the OOB PMT.
`abstract void` | `ProgramAssociationTableManager.removeOutOfBandChangeListener(TableChangeListener listener)` Remove the TableChangeListener object for the OOB PAT.

Overview | Package | Class | Use | Tree | Deprecated | Index | Help

PREV NEXT | FRAMES NO FRAMES